# SDRawDiskInfo Struct Reference

Information associated with an SD Card. More...

`#include <SFBSDRaw.h>`

## Data Fields
u32 | serialNumber
| Card serial number.
u32 | blockCount
| Number of 512 byte blocks in the disk.
u8 | manufacturer
| Manufacturer code, e.g., 2==SanDisk.
u8 | oem [2+1]
| Two byte ASCII OEM code, plus courtesy null.
u8 | product [5+1]
| Five bytes ASCII product code, plus courtesy null.
u8 | revision
| Product revision, as two BCD digits (e.g., 0x32==3.2).
u8 | year
| Year of manufacture (0 means year 2000).
u8 | month
| Month of manufacture (1 means January).
u8 | format
| File format code. Unreliable. One-time writable.
bool | copy
| Contents is original (0) or a copy (1). One-time writable.
bool | writeProtect
| Entire card is permanently write-protected if 1. One-time writable.
bool | writeProtectTemporary
| Entire card is currently write-protected if 1. Rewritable.

## Detailed Description

Information associated with an SD Card.

Read via SDRaw::getInfo(). Writing not currently supported.

The documentation for this struct was generated from the following file:

- src/include/SFBSDRaw.h