# LPC23xx.h

    00001 /******************************************************************************
    00002  *   LPC23xx.h:  Header file for NXP LPC23xx/24xx Family Microprocessors
    00003  *   The header file is the super set of all hardware definition of the
    00004  *   peripherals for the LPC23xx/24xx family microprocessor.
    00005  *
    00006  *   Copyright(C) 2006, NXP Semiconductor
    00007  *   All rights reserved.
    00008  *
    00009  *   History
    00010  *   2005.10.01  ver 1.00    Prelimnary version, first Release
    00011  *
    00012  ******************************************************************************/
    00013
    00014 /* Modified by Martin Thomas */
    00015 /* Modified by David Ackley - generic UART offsets */
    00016
    00017 #ifndef __LPC23xx_H
    00018 #define __LPC23xx_H
    00019
    00020 /* Vectored Interrupt Controller (VIC) */
    00021 #define VIC_BASE_ADDR   0xFFFFF000
    00022 #define VICIRQStatus   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x000))
    00023 #define VICFIQStatus   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x004))
    00024 #define VICRawIntr     (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x008))
    00025 #define VICIntSelect   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x00C))
    00026 #define VICIntEnable   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x010))
    00027 #define VICIntEnClr    (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x014))
    00028 #define VICSoftInt     (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x018))
    00029 #define VICSoftIntClr  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x01C))
    00030 #define VICProtection  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x020))
    00031 #define VICSWPrioMask  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x024))
    00032
    00033 #define VICVectAddr0   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x100))
    00034 #define VICVectAddr1   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x104))
    00035 #define VICVectAddr2   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x108))
    00036 #define VICVectAddr3   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x10C))
    00037 #define VICVectAddr4   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x110))
    00038 #define VICVectAddr5   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x114))
    00039 #define VICVectAddr6   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x118))
    00040 #define VICVectAddr7   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x11C))
    00041 #define VICVectAddr8   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x120))
    00042 #define VICVectAddr9   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x124))
    00043 #define VICVectAddr10  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x128))
    00044 #define VICVectAddr11  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x12C))
    00045 #define VICVectAddr12  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x130))
    00046 #define VICVectAddr13  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x134))
    00047 #define VICVectAddr14  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x138))
    00048 #define VICVectAddr15  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x13C))
    00049 #define VICVectAddr16  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x140))
    00050 #define VICVectAddr17  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x144))
    00051 #define VICVectAddr18  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x148))
    00052 #define VICVectAddr19  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x14C))
    00053 #define VICVectAddr20  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x150))
    00054 #define VICVectAddr21  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x154))
    00055 #define VICVectAddr22  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x158))
    00056 #define VICVectAddr23  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x15C))
    00057 #define VICVectAddr24  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x160))
    00058 #define VICVectAddr25  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x164))
    00059 #define VICVectAddr26  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x168))
    00060 #define VICVectAddr27  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x16C))
    00061 #define VICVectAddr28  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x170))
    00062 #define VICVectAddr29  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x174))
    00063 #define VICVectAddr30  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x178))
    00064 #define VICVectAddr31  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x17C))
    00065
    00066 /* The name convention below is from previous LPC2000 family MCUs, in LPC23xx/24xx,
    00067 these registers are known as "VICVectPriority(x)". */
    00068 #define VICVectCntl0   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x200))
    00069 #define VICVectCntl1   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x204))
    00070 #define VICVectCntl2   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x208))
    00071 #define VICVectCntl3   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x20C))
    00072 #define VICVectCntl4   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x210))
    00073 #define VICVectCntl5   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x214))
    00074 #define VICVectCntl6   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x218))
    00075 #define VICVectCntl7   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x21C))
    00076 #define VICVectCntl8   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x220))
    00077 #define VICVectCntl9   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x224))
    00078 #define VICVectCntl10  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x228))
    00079 #define VICVectCntl11  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x22C))
    00080 #define VICVectCntl12  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x230))
    00081 #define VICVectCntl13  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x234))
    00082 #define VICVectCntl14  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x238))
    00083 #define VICVectCntl15  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x23C))
    00084 #define VICVectCntl16  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x240))
    00085 #define VICVectCntl17  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x244))
    00086 #define VICVectCntl18  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x248))
    00087 #define VICVectCntl19  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x24C))
    00088 #define VICVectCntl20  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x250))
    00089 #define VICVectCntl21  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x254))
    00090 #define VICVectCntl22  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x258))
    00091 #define VICVectCntl23  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x25C))
    00092 #define VICVectCntl24  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x260))
    00093 #define VICVectCntl25  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x264))
    00094 #define VICVectCntl26  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x268))
    00095 #define VICVectCntl27  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x26C))
    00096 #define VICVectCntl28  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x270))
    00097 #define VICVectCntl29  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x274))
    00098 #define VICVectCntl30  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x278))
    00099 #define VICVectCntl31  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x27C))
    00100
    00101 /* mthomas - added "real" names */
    00102 #define VICVectPriority0   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x200))
    00103 #define VICVectPriority1   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x204))
    00104 #define VICVectPriority2   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x208))
    00105 #define VICVectPriority3   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x20C))
    00106 #define VICVectPriority4   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x210))
    00107 #define VICVectPriority5   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x214))
    00108 #define VICVectPriority6   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x218))
    00109 #define VICVectPriority7   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x21C))
    00110 #define VICVectPriority8   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x220))
    00111 #define VICVectPriority9   (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x224))
    00112 #define VICVectPriority10  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x228))
    00113 #define VICVectPriority11  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x22C))
    00114 #define VICVectPriority12  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x230))
    00115 #define VICVectPriority13  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x234))
    00116 #define VICVectPriority14  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x238))
    00117 #define VICVectPriority15  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x23C))
    00118 #define VICVectPriority16  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x240))
    00119 #define VICVectPriority17  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x244))
    00120 #define VICVectPriority18  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x248))
    00121 #define VICVectPriority19  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x24C))
    00122 #define VICVectPriority20  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x250))
    00123 #define VICVectPriority21  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x254))
    00124 #define VICVectPriority22  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x258))
    00125 #define VICVectPriority23  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x25C))
    00126 #define VICVectPriority24  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x260))
    00127 #define VICVectPriority25  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x264))
    00128 #define VICVectPriority26  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x268))
    00129 #define VICVectPriority27  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x26C))
    00130 #define VICVectPriority28  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x270))
    00131 #define VICVectPriority29  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x274))
    00132 #define VICVectPriority30  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x278))
    00133 #define VICVectPriority31  (*(volatile unsigned long *)(VIC_BASE_ADDR + 0x27C))
    00134
    00135
    00136 #define VICVectAddr    (*(volatile unsigned long *)(VIC_BASE_ADDR + 0xF00))
    00137
    00138
    00139 /* Pin Connect Block */
    00140 #define PINSEL_BASE_ADDR        0xE002C000
    00141 #define PINSEL0        (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x00))
    00142 #define PINSEL1        (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x04))
    00143 #define PINSEL2        (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x08))
    00144 #define PINSEL3        (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x0C))
    00145 #define PINSEL4        (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x10))
    00146 #define PINSEL5        (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x14))
    00147 #define PINSEL6        (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x18))
    00148 #define PINSEL7        (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x1C))
    00149 #define PINSEL8        (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x20))
    00150 #define PINSEL9        (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x24))
    00151 #define PINSEL10       (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x28))
    00152
    00153 #define PINMODE_BASE_ADDR       (PINSEL_BASE_ADDR+0x40)
    00154 #define PINMODE0        (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x40))
    00155 #define PINMODE1        (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x44))
    00156 #define PINMODE2        (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x48))
    00157 #define PINMODE3        (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x4C))
    00158 #define PINMODE4        (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x50))
    00159 #define PINMODE5        (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x54))
    00160 #define PINMODE6        (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x58))
    00161 #define PINMODE7        (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x5C))
    00162 #define PINMODE8        (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x60))
    00163 #define PINMODE9        (*(volatile unsigned long *)(PINSEL_BASE_ADDR + 0x64))
    00164
    00165 /* General Purpose Input/Output (GPIO) */
    00166 #define GPIO_BASE_ADDR          0xE0028000
    00167 #define IOPIN0         (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x00))
    00168 #define IOSET0         (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x04))
    00169 #define IODIR0         (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x08))
    00170 #define IOCLR0         (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x0C))
    00171 #define IOPIN1         (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x10))
    00172 #define IOSET1         (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x14))
    00173 #define IODIR1         (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x18))
    00174 #define IOCLR1         (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x1C))
    00175
    00176 /* mthomas - alias */
    00177 #define IO0PIN         (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x00))
    00178 #define IO0SET         (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x04))
    00179 #define IO0DIR         (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x08))
    00180 #define IO0CLR         (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x0C))
    00181 #define IO1PIN         (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x10))
    00182 #define IO1SET         (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x14))
    00183 #define IO1DIR         (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x18))
    00184 #define IO1CLR         (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x1C))
    00185
    00186
    00187 /* GPIO Interrupt Registers */
    00188 #define IO0_INT_EN_R    (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x90))
    00189 #define IO0_INT_EN_F    (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x94))
    00190 #define IO0_INT_STAT_R  (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x84))
    00191 #define IO0_INT_STAT_F  (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x88))
    00192 #define IO0_INT_CLR     (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x8C))
    00193
    00194 #define IO2_INT_EN_R    (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0xB0))
    00195 #define IO2_INT_EN_F    (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0xB4))
    00196 #define IO2_INT_STAT_R  (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0xA4))
    00197 #define IO2_INT_STAT_F  (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0xA8))
    00198 #define IO2_INT_CLR     (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0xAC))
    00199
    00200 #define IO_INT_STAT     (*(volatile unsigned long *)(GPIO_BASE_ADDR + 0x80))
    00201
    00202 #define PARTCFG_BASE_ADDR               0x3FFF8000
    00203 #define PARTCFG        (*(volatile unsigned long *)(PARTCFG_BASE_ADDR + 0x00))
    00204
    00205 /* Fast I/O setup */
    00206 #define FIO_BASE_ADDR           0x3FFFC000
    00207 #define FIO0DIR        (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x00))
    00208 #define FIO0MASK       (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x10))
    00209 #define FIO0PIN        (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x14))
    00210 #define FIO0SET        (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x18))
    00211 #define FIO0CLR        (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x1C))
    00212
    00213 #define FIO1DIR        (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x20))
    00214 #define FIO1MASK       (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x30))
    00215 #define FIO1PIN        (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x34))
    00216 #define FIO1SET        (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x38))
    00217 #define FIO1CLR        (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x3C))
    00218
    00219 #define FIO2DIR        (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x40))
    00220 #define FIO2MASK       (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x50))
    00221 #define FIO2PIN        (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x54))
    00222 #define FIO2SET        (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x58))
    00223 #define FIO2CLR        (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x5C))
    00224
    00225 #define FIO3DIR        (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x60))
    00226 #define FIO3MASK       (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x70))
    00227 #define FIO3PIN        (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x74))
    00228 #define FIO3SET        (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x78))
    00229 #define FIO3CLR        (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x7C))
    00230
    00231 #define FIO4DIR        (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x80))
    00232 #define FIO4MASK       (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x90))
    00233 #define FIO4PIN        (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x94))
    00234 #define FIO4SET        (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x98))
    00235 #define FIO4CLR        (*(volatile unsigned long *)(FIO_BASE_ADDR + 0x9C))
    00236
    00237 /* FIOs can be accessed through WORD, HALF-WORD or BYTE. */
    00238 #define FIO0DIR0       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x00))
    00239 #define FIO1DIR0       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x20))
    00240 #define FIO2DIR0       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x40))
    00241 #define FIO3DIR0       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x60))
    00242 #define FIO4DIR0       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x80))
    00243
    00244 #define FIO0DIR1       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x01))
    00245 #define FIO1DIR1       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x21))
    00246 #define FIO2DIR1       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x41))
    00247 #define FIO3DIR1       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x61))
    00248 #define FIO4DIR1       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x81))
    00249
    00250 #define FIO0DIR2       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x02))
    00251 #define FIO1DIR2       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x22))
    00252 #define FIO2DIR2       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x42))
    00253 #define FIO3DIR2       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x62))
    00254 #define FIO4DIR2       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x82))
    00255
    00256 #define FIO0DIR3       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x03))
    00257 #define FIO1DIR3       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x23))
    00258 #define FIO2DIR3       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x43))
    00259 #define FIO3DIR3       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x63))
    00260 #define FIO4DIR3       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x83))
    00261
    00262 #define FIO0DIRL       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x00))
    00263 #define FIO1DIRL       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x20))
    00264 #define FIO2DIRL       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x40))
    00265 #define FIO3DIRL       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x60))
    00266 #define FIO4DIRL       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x80))
    00267
    00268 #define FIO0DIRU       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x02))
    00269 #define FIO1DIRU       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x22))
    00270 #define FIO2DIRU       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x42))
    00271 #define FIO3DIRU       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x62))
    00272 #define FIO4DIRU       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x82))
    00273
    00274 #define FIO0MASK0      (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x10))
    00275 #define FIO1MASK0      (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x30))
    00276 #define FIO2MASK0      (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x50))
    00277 #define FIO3MASK0      (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x70))
    00278 #define FIO4MASK0      (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x90))
    00279
    00280 #define FIO0MASK1      (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x11))
    00281 #define FIO1MASK1      (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x21))
    00282 #define FIO2MASK1      (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x51))
    00283 #define FIO3MASK1      (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x71))
    00284 #define FIO4MASK1      (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x91))
    00285
    00286 #define FIO0MASK2      (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x12))
    00287 #define FIO1MASK2      (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x32))
    00288 #define FIO2MASK2      (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x52))
    00289 #define FIO3MASK2      (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x72))
    00290 #define FIO4MASK2      (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x92))
    00291
    00292 #define FIO0MASK3      (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x13))
    00293 #define FIO1MASK3      (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x33))
    00294 #define FIO2MASK3      (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x53))
    00295 #define FIO3MASK3      (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x73))
    00296 #define FIO4MASK3      (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x93))
    00297
    00298 #define FIO0MASKL      (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x10))
    00299 #define FIO1MASKL      (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x30))
    00300 #define FIO2MASKL      (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x50))
    00301 #define FIO3MASKL      (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x70))
    00302 #define FIO4MASKL      (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x90))
    00303
    00304 #define FIO0MASKU      (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x12))
    00305 #define FIO1MASKU      (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x32))
    00306 #define FIO2MASKU      (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x52))
    00307 #define FIO3MASKU      (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x72))
    00308 #define FIO4MASKU      (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x92))
    00309
    00310 #define FIO0PIN0       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x14))
    00311 #define FIO1PIN0       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x34))
    00312 #define FIO2PIN0       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x54))
    00313 #define FIO3PIN0       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x74))
    00314 #define FIO4PIN0       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x94))
    00315
    00316 #define FIO0PIN1       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x15))
    00317 #define FIO1PIN1       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x25))
    00318 #define FIO2PIN1       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x55))
    00319 #define FIO3PIN1       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x75))
    00320 #define FIO4PIN1       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x95))
    00321
    00322 #define FIO0PIN2       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x16))
    00323 #define FIO1PIN2       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x36))
    00324 #define FIO2PIN2       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x56))
    00325 #define FIO3PIN2       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x76))
    00326 #define FIO4PIN2       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x96))
    00327
    00328 #define FIO0PIN3       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x17))
    00329 #define FIO1PIN3       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x37))
    00330 #define FIO2PIN3       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x57))
    00331 #define FIO3PIN3       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x77))
    00332 #define FIO4PIN3       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x97))
    00333
    00334 #define FIO0PINL       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x14))
    00335 #define FIO1PINL       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x34))
    00336 #define FIO2PINL       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x54))
    00337 #define FIO3PINL       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x74))
    00338 #define FIO4PINL       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x94))
    00339
    00340 #define FIO0PINU       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x16))
    00341 #define FIO1PINU       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x36))
    00342 #define FIO2PINU       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x56))
    00343 #define FIO3PINU       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x76))
    00344 #define FIO4PINU       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x96))
    00345
    00346 #define FIO0SET0       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x18))
    00347 #define FIO1SET0       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x38))
    00348 #define FIO2SET0       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x58))
    00349 #define FIO3SET0       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x78))
    00350 #define FIO4SET0       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x98))
    00351
    00352 #define FIO0SET1       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x19))
    00353 #define FIO1SET1       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x29))
    00354 #define FIO2SET1       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x59))
    00355 #define FIO3SET1       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x79))
    00356 #define FIO4SET1       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x99))
    00357
    00358 #define FIO0SET2       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x1A))
    00359 #define FIO1SET2       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x3A))
    00360 #define FIO2SET2       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x5A))
    00361 #define FIO3SET2       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x7A))
    00362 #define FIO4SET2       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x9A))
    00363
    00364 #define FIO0SET3       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x1B))
    00365 #define FIO1SET3       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x3B))
    00366 #define FIO2SET3       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x5B))
    00367 #define FIO3SET3       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x7B))
    00368 #define FIO4SET3       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x9B))
    00369
    00370 #define FIO0SETL       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x18))
    00371 #define FIO1SETL       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x38))
    00372 #define FIO2SETL       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x58))
    00373 #define FIO3SETL       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x78))
    00374 #define FIO4SETL       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x98))
    00375
    00376 #define FIO0SETU       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x1A))
    00377 #define FIO1SETU       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x3A))
    00378 #define FIO2SETU       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x5A))
    00379 #define FIO3SETU       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x7A))
    00380 #define FIO4SETU       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x9A))
    00381
    00382 #define FIO0CLR0       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x1C))
    00383 #define FIO1CLR0       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x3C))
    00384 #define FIO2CLR0       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x5C))
    00385 #define FIO3CLR0       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x7C))
    00386 #define FIO4CLR0       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x9C))
    00387
    00388 #define FIO0CLR1       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x1D))
    00389 #define FIO1CLR1       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x2D))
    00390 #define FIO2CLR1       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x5D))
    00391 #define FIO3CLR1       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x7D))
    00392 #define FIO4CLR1       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x9D))
    00393
    00394 #define FIO0CLR2       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x1E))
    00395 #define FIO1CLR2       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x3E))
    00396 #define FIO2CLR2       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x5E))
    00397 #define FIO3CLR2       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x7E))
    00398 #define FIO4CLR2       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x9E))
    00399
    00400 #define FIO0CLR3       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x1F))
    00401 #define FIO1CLR3       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x3F))
    00402 #define FIO2CLR3       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x5F))
    00403 #define FIO3CLR3       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x7F))
    00404 #define FIO4CLR3       (*(volatile unsigned char *)(FIO_BASE_ADDR + 0x9F))
    00405
    00406 #define FIO0CLRL       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x1C))
    00407 #define FIO1CLRL       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x3C))
    00408 #define FIO2CLRL       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x5C))
    00409 #define FIO3CLRL       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x7C))
    00410 #define FIO4CLRL       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x9C))
    00411
    00412 #define FIO0CLRU       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x1E))
    00413 #define FIO1CLRU       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x3E))
    00414 #define FIO2CLRU       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x5E))
    00415 #define FIO3CLRU       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x7E))
    00416 #define FIO4CLRU       (*(volatile unsigned short *)(FIO_BASE_ADDR + 0x9E))
    00417
    00418 /* bit 0 in SCS register, port 0/1 are regular ports when bit 0
    00419 is 0,  fast ports when bit 0 is 1. */
    00420 #define GPIOM         0x00000001
    00421
    00422 /* System Control Block(SCB) modules include Memory Accelerator Module,
    00423 Phase Locked Loop, VPB divider, Power Control, External Interrupt,
    00424 Reset, and Code Security/Debugging */
    00425 #define SCB_BASE_ADDR   0xE01FC000
    00426
    00427 /* Memory Accelerator Module (MAM) */
    00428 #define MAMCR          (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x000))
    00429 #define MAMTIM         (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x004))
    00430 #define MEMMAP         (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x040))
    00431
    00432 /* MEMMAP defines */
    00433 #define MEMMAP_BBLK   0  /* Interrupt Vectors in Boot Block */
    00434 #define MEMMAP_FLASH  1  /* Interrupt Vectors in Flash */
    00435 #define MEMMAP_SRAM   2  /* Interrupt Vectors in SRAM */
    00436
    00437 /* Phase Locked Loop (PLL) */
    00438 #define PLLCON         (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x080))
    00439 #define PLLCFG         (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x084))
    00440 #define PLLSTAT        (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x088))
    00441 #define PLLFEED        (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x08C))
    00442
    00443 /* Power Control */
    00444 #define PCON           (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x0C0))
    00445 #define PCONP          (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x0C4))
    00446
    00447 /* Ackley: Added PCONP bit definitions */
    00448                        /* bit 0 unused */
    00449 #define PCTIM0         (1UL<<1)  /* Timer/counter 0 power/clock control bit */
    00450 #define PCTIM1         (1UL<<2)  /* Timer/counter 1 power/clock control bit */
    00451 #define PCUART0        (1UL<<3)  /* UART0 power/clock control bit */
    00452 #define PCUART1        (1UL<<4)  /* UART1 power/clock control bit */
    00453                        /* bit 5 unused */
    00454 #define PCPWM1         (1UL<<6)  /* PWM1 power/clock control bit */
    00455 #define PCI2C0         (1UL<<7)  /* I2C0 power/clock control bit */
    00456 #define PCSPI          (1UL<<8)  /* SPI power/clock control bit */
    00457 #define PCRTC          (1UL<<9)  /* RTC power/clock control bit */
    00458 #define PCSSP1         (1UL<<10) /* SSP1 power/clock control bit */
    00459 #define PCEMC          (1UL<<11) /* External Memory controller */
    00460 #define PCAD           (1UL<<12) /* A/D converter power/clock control bit (needs special handling) */
    00461 #define PCAN1          (1UL<<13) /* CAN Controller 1 power/clock control bit */
    00462 #define PCAN2          (1UL<<14) /* CAN Controller 2 power/clock control bit */
    00463                        /* bit 15 unused */
    00464                        /* bit 16 unused */
    00465                        /* bit 17 unused */
    00466                        /* bit 18 unused */
    00467 #define PCI2C1         (1UL<<19) /* I2C1 power/clock control bit */
    00468                        /* bit 20 unused */
    00469 #define PCSSP0         (1UL<<21) /* SSP0 power/clock control bit */
    00470 #define PCTIM2         (1UL<<22) /* Timer 2 power/clock control bit */
    00471 #define PCTIM3         (1UL<<23) /* Timer 3 power/clock control bit */
    00472 #define PCUART2        (1UL<<24) /* UART2 power/clock control bit */
    00473 #define PCUART3        (1UL<<25) /* UART3 power/clock control bit */
    00474 #define PCI2C2         (1UL<<26) /* I2C2 power/clock control bit */
    00475 #define PCI2S          (1UL<<27) /* I2S power/clock control bit */
    00476 #define PCSDC          (1UL<<28) /* SD card power/clock control bit */
    00477 #define PCGPDMA        (1UL<<29) /* GP DMA power/clock control bit */
    00478 #define PCENET         (1UL<<30) /* Ethernet power/clock control bit */
    00479 #define PCUSB          (1UL<<31) /* USB power/clock control bit */
    00480
    00481 /* Clock Divider */
    00482 /* #define APBDIV         (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x100)) */
    00483 #define CCLKCFG        (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x104))
    00484 #define USBCLKCFG      (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x108))
    00485 #define CLKSRCSEL      (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x10C))
    00486 #define PCLKSEL0       (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x1A8))
    00487 #define PCLKSEL1       (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x1AC))
    00488
    00489 /* External Interrupts */
    00490 #define EXTINT         (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x140))
    00491 #define INTWAKE        (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x144))
    00492 #define EXTMODE        (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x148))
    00493 #define EXTPOLAR       (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x14C))
    00494
    00495 /* Reset, reset source identification */
    00496 #define RSIR           (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x180))
    00497
    00498 /* RSID, code security protection */
    00499 #define CSPR           (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x184))
    00500
    00501 /* AHB configuration */
    00502 #define AHBCFG1        (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x188))
    00503 #define AHBCFG2        (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x18C))
    00504
    00505 /* System Controls and Status */
    00506 #define SCS            (*(volatile unsigned long *)(SCB_BASE_ADDR + 0x1A0))
    00507
    00508 /* MPMC(EMC) registers, note: all the external memory controller(EMC) registers
    00509 are for LPC24xx only. */
    00510 #define STATIC_MEM0_BASE                0x80000000
    00511 #define STATIC_MEM1_BASE                0x81000000
    00512 #define STATIC_MEM2_BASE                0x82000000
    00513 #define STATIC_MEM3_BASE                0x83000000
    00514
    00515 #define DYNAMIC_MEM0_BASE               0xA0000000
    00516 #define DYNAMIC_MEM1_BASE               0xB0000000
    00517 #define DYNAMIC_MEM2_BASE               0xC0000000
    00518 #define DYNAMIC_MEM3_BASE               0xD0000000
    00519
    00520 /* External Memory Controller (EMC) */
    00521 #define EMC_BASE_ADDR           0xFFE08000
    00522 #define EMC_CTRL       (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x000))
    00523 #define EMC_STAT       (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x004))
    00524 #define EMC_CONFIG     (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x008))
    00525
    00526 /* Dynamic RAM access registers */
    00527 #define EMC_DYN_CTRL     (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x020))
    00528 #define EMC_DYN_RFSH     (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x024))
    00529 #define EMC_DYN_RD_CFG   (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x028))
    00530 #define EMC_DYN_RP       (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x030))
    00531 #define EMC_DYN_RAS      (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x034))
    00532 #define EMC_DYN_SREX     (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x038))
    00533 #define EMC_DYN_APR      (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x03C))
    00534 #define EMC_DYN_DAL      (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x040))
    00535 #define EMC_DYN_WR       (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x044))
    00536 #define EMC_DYN_RC       (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x048))
    00537 #define EMC_DYN_RFC      (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x04C))
    00538 #define EMC_DYN_XSR      (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x050))
    00539 #define EMC_DYN_RRD      (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x054))
    00540 #define EMC_DYN_MRD      (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x058))
    00541
    00542 #define EMC_DYN_CFG0     (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x100))
    00543 #define EMC_DYN_RASCAS0  (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x104))
    00544 #define EMC_DYN_CFG1     (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x140))
    00545 #define EMC_DYN_RASCAS1  (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x144))
    00546 #define EMC_DYN_CFG2     (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x160))
    00547 #define EMC_DYN_RASCAS2  (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x164))
    00548 #define EMC_DYN_CFG3     (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x180))
    00549 #define EMC_DYN_RASCAS3  (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x184))
    00550
    00551 /* static RAM access registers */
    00552 #define EMC_STA_CFG0      (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x200))
    00553 #define EMC_STA_WAITWEN0  (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x204))
    00554 #define EMC_STA_WAITOEN0  (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x208))
    00555 #define EMC_STA_WAITRD0   (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x20C))
    00556 #define EMC_STA_WAITPAGE0 (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x210))
    00557 #define EMC_STA_WAITWR0   (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x214))
    00558 #define EMC_STA_WAITTURN0 (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x218))
    00559
    00560 #define EMC_STA_CFG1      (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x220))
    00561 #define EMC_STA_WAITWEN1  (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x224))
    00562 #define EMC_STA_WAITOEN1  (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x228))
    00563 #define EMC_STA_WAITRD1   (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x22C))
    00564 #define EMC_STA_WAITPAGE1 (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x230))
    00565 #define EMC_STA_WAITWR1   (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x234))
    00566 #define EMC_STA_WAITTURN1 (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x238))
    00567
    00568 #define EMC_STA_CFG2      (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x240))
    00569 #define EMC_STA_WAITWEN2  (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x244))
    00570 #define EMC_STA_WAITOEN2  (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x248))
    00571 #define EMC_STA_WAITRD2   (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x24C))
    00572 #define EMC_STA_WAITPAGE2 (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x250))
    00573 #define EMC_STA_WAITWR2   (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x254))
    00574 #define EMC_STA_WAITTURN2 (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x258))
    00575
    00576 #define EMC_STA_CFG3      (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x260))
    00577 #define EMC_STA_WAITWEN3  (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x264))
    00578 #define EMC_STA_WAITOEN3  (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x268))
    00579 #define EMC_STA_WAITRD3   (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x26C))
    00580 #define EMC_STA_WAITPAGE3 (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x270))
    00581 #define EMC_STA_WAITWR3   (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x274))
    00582 #define EMC_STA_WAITTURN3 (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x278))
    00583
    00584 #define EMC_STA_EXT_WAIT  (*(volatile unsigned long *)(EMC_BASE_ADDR + 0x880))
    00585
    00586
    00587 /* Timer 0 */
    00588 #define TMR0_BASE_ADDR          0xE0004000
    00589 #define T0IR           (*(volatile unsigned long *)(TMR0_BASE_ADDR + 0x00))
    00590 #define T0TCR          (*(volatile unsigned long *)(TMR0_BASE_ADDR + 0x04))
    00591 #define T0TC           (*(volatile unsigned long *)(TMR0_BASE_ADDR + 0x08))
    00592 #define T0PR           (*(volatile unsigned long *)(TMR0_BASE_ADDR + 0x0C))
    00593 #define T0PC           (*(volatile unsigned long *)(TMR0_BASE_ADDR + 0x10))
    00594 #define T0MCR          (*(volatile unsigned long *)(TMR0_BASE_ADDR + 0x14))
    00595 #define T0MR0          (*(volatile unsigned long *)(TMR0_BASE_ADDR + 0x18))
    00596 #define T0MR1          (*(volatile unsigned long *)(TMR0_BASE_ADDR + 0x1C))
    00597 #define T0MR2          (*(volatile unsigned long *)(TMR0_BASE_ADDR + 0x20))
    00598 #define T0MR3          (*(volatile unsigned long *)(TMR0_BASE_ADDR + 0x24))
    00599 #define T0CCR          (*(volatile unsigned long *)(TMR0_BASE_ADDR + 0x28))
    00600 #define T0CR0          (*(volatile unsigned long *)(TMR0_BASE_ADDR + 0x2C))
    00601 #define T0CR1          (*(volatile unsigned long *)(TMR0_BASE_ADDR + 0x30))
    00602 #define T0CR2          (*(volatile unsigned long *)(TMR0_BASE_ADDR + 0x34))
    00603 #define T0CR3          (*(volatile unsigned long *)(TMR0_BASE_ADDR + 0x38))
    00604 #define T0EMR          (*(volatile unsigned long *)(TMR0_BASE_ADDR + 0x3C))
    00605 #define T0CTCR         (*(volatile unsigned long *)(TMR0_BASE_ADDR + 0x70))
    00606
    00607 /* Timer 1 */
    00608 #define TMR1_BASE_ADDR          0xE0008000
    00609 #define T1IR           (*(volatile unsigned long *)(TMR1_BASE_ADDR + 0x00))
    00610 #define T1TCR          (*(volatile unsigned long *)(TMR1_BASE_ADDR + 0x04))
    00611 #define T1TC           (*(volatile unsigned long *)(TMR1_BASE_ADDR + 0x08))
    00612 #define T1PR           (*(volatile unsigned long *)(TMR1_BASE_ADDR + 0x0C))
    00613 #define T1PC           (*(volatile unsigned long *)(TMR1_BASE_ADDR + 0x10))
    00614 #define T1MCR          (*(volatile unsigned long *)(TMR1_BASE_ADDR + 0x14))
    00615 #define T1MR0          (*(volatile unsigned long *)(TMR1_BASE_ADDR + 0x18))
    00616 #define T1MR1          (*(volatile unsigned long *)(TMR1_BASE_ADDR + 0x1C))
    00617 #define T1MR2          (*(volatile unsigned long *)(TMR1_BASE_ADDR + 0x20))
    00618 #define T1MR3          (*(volatile unsigned long *)(TMR1_BASE_ADDR + 0x24))
    00619 #define T1CCR          (*(volatile unsigned long *)(TMR1_BASE_ADDR + 0x28))
    00620 #define T1CR0          (*(volatile unsigned long *)(TMR1_BASE_ADDR + 0x2C))
    00621 #define T1CR1          (*(volatile unsigned long *)(TMR1_BASE_ADDR + 0x30))
    00622 #define T1CR2          (*(volatile unsigned long *)(TMR1_BASE_ADDR + 0x34))
    00623 #define T1CR3          (*(volatile unsigned long *)(TMR1_BASE_ADDR + 0x38))
    00624 #define T1EMR          (*(volatile unsigned long *)(TMR1_BASE_ADDR + 0x3C))
    00625 #define T1CTCR         (*(volatile unsigned long *)(TMR1_BASE_ADDR + 0x70))
    00626
    00627 /* Timer 2 */
    00628 #define TMR2_BASE_ADDR          0xE0070000
    00629 #define T2IR           (*(volatile unsigned long *)(TMR2_BASE_ADDR + 0x00))
    00630 #define T2TCR          (*(volatile unsigned long *)(TMR2_BASE_ADDR + 0x04))
    00631 #define T2TC           (*(volatile unsigned long *)(TMR2_BASE_ADDR + 0x08))
    00632 #define T2PR           (*(volatile unsigned long *)(TMR2_BASE_ADDR + 0x0C))
    00633 #define T2PC           (*(volatile unsigned long *)(TMR2_BASE_ADDR + 0x10))
    00634 #define T2MCR          (*(volatile unsigned long *)(TMR2_BASE_ADDR + 0x14))
    00635 #define T2MR0          (*(volatile unsigned long *)(TMR2_BASE_ADDR + 0x18))
    00636 #define T2MR1          (*(volatile unsigned long *)(TMR2_BASE_ADDR + 0x1C))
    00637 #define T2MR2          (*(volatile unsigned long *)(TMR2_BASE_ADDR + 0x20))
    00638 #define T2MR3          (*(volatile unsigned long *)(TMR2_BASE_ADDR + 0x24))
    00639 #define T2CCR          (*(volatile unsigned long *)(TMR2_BASE_ADDR + 0x28))
    00640 #define T2CR0          (*(volatile unsigned long *)(TMR2_BASE_ADDR + 0x2C))
    00641 #define T2CR1          (*(volatile unsigned long *)(TMR2_BASE_ADDR + 0x30))
    00642 #define T2CR2          (*(volatile unsigned long *)(TMR2_BASE_ADDR + 0x34))
    00643 #define T2CR3          (*(volatile unsigned long *)(TMR2_BASE_ADDR + 0x38))
    00644 #define T2EMR          (*(volatile unsigned long *)(TMR2_BASE_ADDR + 0x3C))
    00645 #define T2CTCR         (*(volatile unsigned long *)(TMR2_BASE_ADDR + 0x70))
    00646
    00647 /* Timer 3 */
    00648 #define TMR3_BASE_ADDR          0xE0074000
    00649 #define T3IR           (*(volatile unsigned long *)(TMR3_BASE_ADDR + 0x00))
    00650 #define T3TCR          (*(volatile unsigned long *)(TMR3_BASE_ADDR + 0x04))
    00651 #define T3TC           (*(volatile unsigned long *)(TMR3_BASE_ADDR + 0x08))
    00652 #define T3PR           (*(volatile unsigned long *)(TMR3_BASE_ADDR + 0x0C))
    00653 #define T3PC           (*(volatile unsigned long *)(TMR3_BASE_ADDR + 0x10))
    00654 #define T3MCR          (*(volatile unsigned long *)(TMR3_BASE_ADDR + 0x14))
    00655 #define T3MR0          (*(volatile unsigned long *)(TMR3_BASE_ADDR + 0x18))
    00656 #define T3MR1          (*(volatile unsigned long *)(TMR3_BASE_ADDR + 0x1C))
    00657 #define T3MR2          (*(volatile unsigned long *)(TMR3_BASE_ADDR + 0x20))
    00658 #define T3MR3          (*(volatile unsigned long *)(TMR3_BASE_ADDR + 0x24))
    00659 #define T3CCR          (*(volatile unsigned long *)(TMR3_BASE_ADDR + 0x28))
    00660 #define T3CR0          (*(volatile unsigned long *)(TMR3_BASE_ADDR + 0x2C))
    00661 #define T3CR1          (*(volatile unsigned long *)(TMR3_BASE_ADDR + 0x30))
    00662 #define T3CR2          (*(volatile unsigned long *)(TMR3_BASE_ADDR + 0x34))
    00663 #define T3CR3          (*(volatile unsigned long *)(TMR3_BASE_ADDR + 0x38))
    00664 #define T3EMR          (*(volatile unsigned long *)(TMR3_BASE_ADDR + 0x3C))
    00665 #define T3CTCR         (*(volatile unsigned long *)(TMR3_BASE_ADDR + 0x70))
    00666
    00667 /* Pulse Width Modulator (PWM) */
    00668 #define PWM0_BASE_ADDR          0xE0014000
    00669 #define PWM0IR          (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x00))
    00670 #define PWM0TCR         (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x04))
    00671 #define PWM0TC          (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x08))
    00672 #define PWM0PR          (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x0C))
    00673 #define PWM0PC          (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x10))
    00674 #define PWM0MCR         (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x14))
    00675 #define PWM0MR0         (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x18))
    00676 #define PWM0MR1         (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x1C))
    00677 #define PWM0MR2         (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x20))
    00678 #define PWM0MR3         (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x24))
    00679 #define PWM0CCR         (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x28))
    00680 #define PWM0CR0         (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x2C))
    00681 #define PWM0CR1         (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x30))
    00682 #define PWM0CR2         (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x34))
    00683 #define PWM0CR3         (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x38))
    00684 #define PWM0EMR         (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x3C))
    00685 #define PWM0MR4         (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x40))
    00686 #define PWM0MR5         (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x44))
    00687 #define PWM0MR6         (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x48))
    00688 #define PWM0PCR         (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x4C))
    00689 #define PWM0LER         (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x50))
    00690 #define PWM0CTCR        (*(volatile unsigned long *)(PWM0_BASE_ADDR + 0x70))
    00691
    00692 #define PWM1_BASE_ADDR          0xE0018000
    00693 #define PWM1IR          (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x00))
    00694 #define PWM1TCR         (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x04))
    00695 #define PWM1TC          (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x08))
    00696 #define PWM1PR          (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x0C))
    00697 #define PWM1PC          (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x10))
    00698 #define PWM1MCR         (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x14))
    00699 #define PWM1MR0         (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x18))
    00700 #define PWM1MR1         (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x1C))
    00701 #define PWM1MR2         (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x20))
    00702 #define PWM1MR3         (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x24))
    00703 #define PWM1CCR         (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x28))
    00704 #define PWM1CR0         (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x2C))
    00705 #define PWM1CR1         (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x30))
    00706 #define PWM1CR2         (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x34))
    00707 #define PWM1CR3         (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x38))
    00708 #define PWM1EMR         (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x3C))
    00709 #define PWM1MR4         (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x40))
    00710 #define PWM1MR5         (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x44))
    00711 #define PWM1MR6         (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x48))
    00712 #define PWM1PCR         (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x4C))
    00713 #define PWM1LER         (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x50))
    00714 #define PWM1CTCR        (*(volatile unsigned long *)(PWM1_BASE_ADDR + 0x70))
    00715
    00716 /* Ackley: Added Generic UART offsets */
    00717 #define UxRBR          0x00
    00718 #define UxTHR          0x00
    00719 #define UxDLL          0x00
    00720 #define UxDLM          0x04
    00721 #define UxIER          0x04
    00722 #define UxIIR          0x08
    00723 #define UxFCR          0x08
    00724 #define UxLCR          0x0C
    00725 #define UxLSR          0x14
    00726 #define UxSCR          0x1C
    00727 #define UxACR          0x20
    00728 #define UxICR          0x24
    00729 #define UxFDR          0x28
    00730 #define UxTER          0x30
    00731
    00732 /* Universal Asynchronous Receiver Transmitter 0 (UART0) */
    00733 #define UART0_BASE_ADDR         0xE000C000
    00734 #define U0RBR          (*(volatile unsigned long *)(UART0_BASE_ADDR + 0x00))
    00735 #define U0THR          (*(volatile unsigned long *)(UART0_BASE_ADDR + 0x00))
    00736 #define U0DLL          (*(volatile unsigned long *)(UART0_BASE_ADDR + 0x00))
    00737 #define U0DLM          (*(volatile unsigned long *)(UART0_BASE_ADDR + 0x04))
    00738 #define U0IER          (*(volatile unsigned long *)(UART0_BASE_ADDR + 0x04))
    00739 #define U0IIR          (*(volatile unsigned long *)(UART0_BASE_ADDR + 0x08))
    00740 #define U0FCR          (*(volatile unsigned long *)(UART0_BASE_ADDR + 0x08))
    00741 #define U0LCR          (*(volatile unsigned long *)(UART0_BASE_ADDR + 0x0C))
    00742 #define U0LSR          (*(volatile unsigned long *)(UART0_BASE_ADDR + 0x14))
    00743 #define U0SCR          (*(volatile unsigned long *)(UART0_BASE_ADDR + 0x1C))
    00744 #define U0ACR          (*(volatile unsigned long *)(UART0_BASE_ADDR + 0x20))
    00745 #define U0ICR          (*(volatile unsigned long *)(UART0_BASE_ADDR + 0x24))
    00746 #define U0FDR          (*(volatile unsigned long *)(UART0_BASE_ADDR + 0x28))
    00747 #define U0TER          (*(volatile unsigned long *)(UART0_BASE_ADDR + 0x30))
    00748
    00749 /* Universal Asynchronous Receiver Transmitter 1 (UART1) */
    00750 #define UART1_BASE_ADDR         0xE0010000
    00751 #define U1RBR          (*(volatile unsigned long *)(UART1_BASE_ADDR + 0x00))
    00752 #define U1THR          (*(volatile unsigned long *)(UART1_BASE_ADDR + 0x00))
    00753 #define U1DLL          (*(volatile unsigned long *)(UART1_BASE_ADDR + 0x00))
    00754 #define U1DLM          (*(volatile unsigned long *)(UART1_BASE_ADDR + 0x04))
    00755 #define U1IER          (*(volatile unsigned long *)(UART1_BASE_ADDR + 0x04))
    00756 #define U1IIR          (*(volatile unsigned long *)(UART1_BASE_ADDR + 0x08))
    00757 #define U1FCR          (*(volatile unsigned long *)(UART1_BASE_ADDR + 0x08))
    00758 #define U1LCR          (*(volatile unsigned long *)(UART1_BASE_ADDR + 0x0C))
    00759 #define U1MCR          (*(volatile unsigned long *)(UART1_BASE_ADDR + 0x10))
    00760 #define U1LSR          (*(volatile unsigned long *)(UART1_BASE_ADDR + 0x14))
    00761 #define U1MSR          (*(volatile unsigned long *)(UART1_BASE_ADDR + 0x18))
    00762 #define U1SCR          (*(volatile unsigned long *)(UART1_BASE_ADDR + 0x1C))
    00763 #define U1ACR          (*(volatile unsigned long *)(UART1_BASE_ADDR + 0x20))
    00764 /*#define U1ICR          (*(volatile unsigned long *)(UART1_BASE_ADDR + 0x24)) ACKLEY -- Only this one was missing from the file, why? */
    00765 #define U1FDR          (*(volatile unsigned long *)(UART1_BASE_ADDR + 0x28))
    00766 #define U1TER          (*(volatile unsigned long *)(UART1_BASE_ADDR + 0x30))
    00767
    00768 /* Universal Asynchronous Receiver Transmitter 2 (UART2) */
    00769 #define UART2_BASE_ADDR         0xE0078000
    00770 #define U2RBR          (*(volatile unsigned long *)(UART2_BASE_ADDR + 0x00))
    00771 #define U2THR          (*(volatile unsigned long *)(UART2_BASE_ADDR + 0x00))
    00772 #define U2DLL          (*(volatile unsigned long *)(UART2_BASE_ADDR + 0x00))
    00773 #define U2DLM          (*(volatile unsigned long *)(UART2_BASE_ADDR + 0x04))
    00774 #define U2IER          (*(volatile unsigned long *)(UART2_BASE_ADDR + 0x04))
    00775 #define U2IIR          (*(volatile unsigned long *)(UART2_BASE_ADDR + 0x08))
    00776 #define U2FCR          (*(volatile unsigned long *)(UART2_BASE_ADDR + 0x08))
    00777 #define U2LCR          (*(volatile unsigned long *)(UART2_BASE_ADDR + 0x0C))
    00778 #define U2LSR          (*(volatile unsigned long *)(UART2_BASE_ADDR + 0x14))
    00779 #define U2SCR          (*(volatile unsigned long *)(UART2_BASE_ADDR + 0x1C))
    00780 #define U2ACR          (*(volatile unsigned long *)(UART2_BASE_ADDR + 0x20))
    00781 #define U2ICR          (*(volatile unsigned long *)(UART2_BASE_ADDR + 0x24))
    00782 #define U2FDR          (*(volatile unsigned long *)(UART2_BASE_ADDR + 0x28))
    00783 #define U2TER          (*(volatile unsigned long *)(UART2_BASE_ADDR + 0x30))
    00784
    00785 /* Universal Asynchronous Receiver Transmitter 3 (UART3) */
    00786 #define UART3_BASE_ADDR         0xE007C000
    00787 #define U3RBR          (*(volatile unsigned long *)(UART3_BASE_ADDR + 0x00))
    00788 #define U3THR          (*(volatile unsigned long *)(UART3_BASE_ADDR + 0x00))
    00789 #define U3DLL          (*(volatile unsigned long *)(UART3_BASE_ADDR + 0x00))
    00790 #define U3DLM          (*(volatile unsigned long *)(UART3_BASE_ADDR + 0x04))
    00791 #define U3IER          (*(volatile unsigned long *)(UART3_BASE_ADDR + 0x04))
    00792 #define U3IIR          (*(volatile unsigned long *)(UART3_BASE_ADDR + 0x08))
    00793 #define U3FCR          (*(volatile unsigned long *)(UART3_BASE_ADDR + 0x08))
    00794 #define U3LCR          (*(volatile unsigned long *)(UART3_BASE_ADDR + 0x0C))
    00795 #define U3LSR          (*(volatile unsigned long *)(UART3_BASE_ADDR + 0x14))
    00796 #define U3SCR          (*(volatile unsigned long *)(UART3_BASE_ADDR + 0x1C))
    00797 #define U3ACR          (*(volatile unsigned long *)(UART3_BASE_ADDR + 0x20))
    00798 #define U3ICR          (*(volatile unsigned long *)(UART3_BASE_ADDR + 0x24))
    00799 #define U3FDR          (*(volatile unsigned long *)(UART3_BASE_ADDR + 0x28))
    00800 #define U3TER          (*(volatile unsigned long *)(UART3_BASE_ADDR + 0x30))
    00801
    00802 /* I2C Interface 0 */
    00803 #define I2C0_BASE_ADDR          0xE001C000
    00804 #define I20CONSET      (*(volatile unsigned long *)(I2C0_BASE_ADDR + 0x00))
    00805 #define I20STAT        (*(volatile unsigned long *)(I2C0_BASE_ADDR + 0x04))
    00806 #define I20DAT         (*(volatile unsigned long *)(I2C0_BASE_ADDR + 0x08))
    00807 #define I20ADR         (*(volatile unsigned long *)(I2C0_BASE_ADDR + 0x0C))
    00808 #define I20SCLH        (*(volatile unsigned long *)(I2C0_BASE_ADDR + 0x10))
    00809 #define I20SCLL        (*(volatile unsigned long *)(I2C0_BASE_ADDR + 0x14))
    00810 #define I20CONCLR      (*(volatile unsigned long *)(I2C0_BASE_ADDR + 0x18))
    00811
    00812 /* I2C Interface 1 */
    00813 #define I2C1_BASE_ADDR          0xE005C000
    00814 #define I21CONSET      (*(volatile unsigned long *)(I2C1_BASE_ADDR + 0x00))
    00815 #define I21STAT        (*(volatile unsigned long *)(I2C1_BASE_ADDR + 0x04))
    00816 #define I21DAT         (*(volatile unsigned long *)(I2C1_BASE_ADDR + 0x08))
    00817 #define I21ADR         (*(volatile unsigned long *)(I2C1_BASE_ADDR + 0x0C))
    00818 #define I21SCLH        (*(volatile unsigned long *)(I2C1_BASE_ADDR + 0x10))
    00819 #define I21SCLL        (*(volatile unsigned long *)(I2C1_BASE_ADDR + 0x14))
    00820 #define I21CONCLR      (*(volatile unsigned long *)(I2C1_BASE_ADDR + 0x18))
    00821
    00822 /* I2C Interface 2 */
    00823 #define I2C2_BASE_ADDR          0xE0080000
    00824 #define I22CONSET      (*(volatile unsigned long *)(I2C2_BASE_ADDR + 0x00))
    00825 #define I22STAT        (*(volatile unsigned long *)(I2C2_BASE_ADDR + 0x04))
    00826 #define I22DAT         (*(volatile unsigned long *)(I2C2_BASE_ADDR + 0x08))
    00827 #define I22ADR         (*(volatile unsigned long *)(I2C2_BASE_ADDR + 0x0C))
    00828 #define I22SCLH        (*(volatile unsigned long *)(I2C2_BASE_ADDR + 0x10))
    00829 #define I22SCLL        (*(volatile unsigned long *)(I2C2_BASE_ADDR + 0x14))
    00830 #define I22CONCLR      (*(volatile unsigned long *)(I2C2_BASE_ADDR + 0x18))
    00831
    00832 /* SPI0 (Serial Peripheral Interface 0) */
    00833 #define SPI0_BASE_ADDR          0xE0020000
    00834 #define S0SPCR         (*(volatile unsigned long *)(SPI0_BASE_ADDR + 0x00))
    00835 #define S0SPSR         (*(volatile unsigned long *)(SPI0_BASE_ADDR + 0x04))
    00836 #define S0SPDR         (*(volatile unsigned long *)(SPI0_BASE_ADDR + 0x08))
    00837 #define S0SPCCR        (*(volatile unsigned long *)(SPI0_BASE_ADDR + 0x0C))
    00838 #define S0SPINT        (*(volatile unsigned long *)(SPI0_BASE_ADDR + 0x1C))
    00839
    00840 /* SSP0 Controller */
    00841 #define SSP0_BASE_ADDR          0xE0068000
    00842 #define SSP0CR0        (*(volatile unsigned long *)(SSP0_BASE_ADDR + 0x00))
    00843 #define SSP0CR1        (*(volatile unsigned long *)(SSP0_BASE_ADDR + 0x04))
    00844 #define SSP0DR         (*(volatile unsigned long *)(SSP0_BASE_ADDR + 0x08))
    00845 #define SSP0SR         (*(volatile unsigned long *)(SSP0_BASE_ADDR + 0x0C))
    00846 #define SSP0CPSR       (*(volatile unsigned long *)(SSP0_BASE_ADDR + 0x10))
    00847 #define SSP0IMSC       (*(volatile unsigned long *)(SSP0_BASE_ADDR + 0x14))
    00848 #define SSP0RIS        (*(volatile unsigned long *)(SSP0_BASE_ADDR + 0x18))
    00849 #define SSP0MIS        (*(volatile unsigned long *)(SSP0_BASE_ADDR + 0x1C))
    00850 #define SSP0ICR        (*(volatile unsigned long *)(SSP0_BASE_ADDR + 0x20))
    00851 #define SSP0DMACR      (*(volatile unsigned long *)(SSP0_BASE_ADDR + 0x24))
    00852
    00853 /* SSP1 Controller */
    00854 #define SSP1_BASE_ADDR          0xE0030000
    00855 #define SSP1CR0        (*(volatile unsigned long *)(SSP1_BASE_ADDR + 0x00))
    00856 #define SSP1CR1        (*(volatile unsigned long *)(SSP1_BASE_ADDR + 0x04))
    00857 #define SSP1DR         (*(volatile unsigned long *)(SSP1_BASE_ADDR + 0x08))
    00858 #define SSP1SR         (*(volatile unsigned long *)(SSP1_BASE_ADDR + 0x0C))
    00859 #define SSP1CPSR       (*(volatile unsigned long *)(SSP1_BASE_ADDR + 0x10))
    00860 #define SSP1IMSC       (*(volatile unsigned long *)(SSP1_BASE_ADDR + 0x14))
    00861 #define SSP1RIS        (*(volatile unsigned long *)(SSP1_BASE_ADDR + 0x18))
    00862 #define SSP1MIS        (*(volatile unsigned long *)(SSP1_BASE_ADDR + 0x1C))
    00863 #define SSP1ICR        (*(volatile unsigned long *)(SSP1_BASE_ADDR + 0x20))
    00864 #define SSP1DMACR      (*(volatile unsigned long *)(SSP1_BASE_ADDR + 0x24))
    00865
    00866
    00867 /* Real Time Clock */
    00868 #define RTC_BASE_ADDR           0xE0024000
    00869 #define RTC_ILR         (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x00))
    00870 #define RTC_CTC         (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x04))
    00871 #define RTC_CCR         (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x08))
    00872 #define RTC_CIIR        (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x0C))
    00873 #define RTC_AMR         (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x10))
    00874 #define RTC_CTIME0      (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x14))
    00875 #define RTC_CTIME1      (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x18))
    00876 #define RTC_CTIME2      (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x1C))
    00877 #define RTC_SEC         (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x20))
    00878 #define RTC_MIN         (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x24))
    00879 #define RTC_HOUR        (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x28))
    00880 #define RTC_DOM         (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x2C))
    00881 #define RTC_DOW         (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x30))
    00882 #define RTC_DOY         (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x34))
    00883 #define RTC_MONTH       (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x38))
    00884 #define RTC_YEAR        (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x3C))
    00885 #define RTC_CISS        (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x40))
    00886 #define RTC_ALSEC       (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x60))
    00887 #define RTC_ALMIN       (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x64))
    00888 #define RTC_ALHOUR      (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x68))
    00889 #define RTC_ALDOM       (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x6C))
    00890 #define RTC_ALDOW       (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x70))
    00891 #define RTC_ALDOY       (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x74))
    00892 #define RTC_ALMON       (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x78))
    00893 #define RTC_ALYEAR      (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x7C))
    00894 #define RTC_PREINT      (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x80))
    00895 #define RTC_PREFRAC     (*(volatile unsigned long *)(RTC_BASE_ADDR + 0x84))
    00896
    00897
    00898 /* A/D Converter 0 (AD0) */
    00899 #define AD0_BASE_ADDR           0xE0034000
    00900 #define AD0CR          (*(volatile unsigned long *)(AD0_BASE_ADDR + 0x00))
    00901 #define AD0GDR         (*(volatile unsigned long *)(AD0_BASE_ADDR + 0x04))
    00902 #define AD0INTEN       (*(volatile unsigned long *)(AD0_BASE_ADDR + 0x0C))
    00903 #define AD0DR0         (*(volatile unsigned long *)(AD0_BASE_ADDR + 0x10))
    00904 #define AD0DR1         (*(volatile unsigned long *)(AD0_BASE_ADDR + 0x14))
    00905 #define AD0DR2         (*(volatile unsigned long *)(AD0_BASE_ADDR + 0x18))
    00906 #define AD0DR3         (*(volatile unsigned long *)(AD0_BASE_ADDR + 0x1C))
    00907 #define AD0DR4         (*(volatile unsigned long *)(AD0_BASE_ADDR + 0x20))
    00908 #define AD0DR5         (*(volatile unsigned long *)(AD0_BASE_ADDR + 0x24))
    00909 #define AD0DR6         (*(volatile unsigned long *)(AD0_BASE_ADDR + 0x28))
    00910 #define AD0DR7         (*(volatile unsigned long *)(AD0_BASE_ADDR + 0x2C))
    00911 #define AD0STAT        (*(volatile unsigned long *)(AD0_BASE_ADDR + 0x30))
    00912
    00913
    00914 /* D/A Converter */
    00915 #define DAC_BASE_ADDR           0xE006C000
    00916 #define DACR           (*(volatile unsigned long *)(DAC_BASE_ADDR + 0x00))
    00917
    00918
    00919 /* Watchdog */
    00920 #define WDG_BASE_ADDR           0xE0000000
    00921 #define WDMOD          (*(volatile unsigned long *)(WDG_BASE_ADDR + 0x00))
    00922 #define WDTC           (*(volatile unsigned long *)(WDG_BASE_ADDR + 0x04))
    00923 #define WDFEED         (*(volatile unsigned long *)(WDG_BASE_ADDR + 0x08))
    00924 #define WDTV           (*(volatile unsigned long *)(WDG_BASE_ADDR + 0x0C))
    00925 #define WDCLKSEL       (*(volatile unsigned long *)(WDG_BASE_ADDR + 0x10))
    00926
    00927 /* CAN CONTROLLERS AND ACCEPTANCE FILTER */
    00928 #define CAN_ACCEPT_BASE_ADDR            0xE003C000
    00929 #define CAN_AFMR                (*(volatile unsigned long *)(CAN_ACCEPT_BASE_ADDR + 0x00))
    00930 #define CAN_SFF_SA              (*(volatile unsigned long *)(CAN_ACCEPT_BASE_ADDR + 0x04))
    00931 #define CAN_SFF_GRP_SA  (*(volatile unsigned long *)(CAN_ACCEPT_BASE_ADDR + 0x08))
    00932 #define CAN_EFF_SA              (*(volatile unsigned long *)(CAN_ACCEPT_BASE_ADDR + 0x0C))
    00933 #define CAN_EFF_GRP_SA  (*(volatile unsigned long *)(CAN_ACCEPT_BASE_ADDR + 0x10))
    00934 #define CAN_EOT                 (*(volatile unsigned long *)(CAN_ACCEPT_BASE_ADDR + 0x14))
    00935 #define CAN_LUT_ERR_ADR (*(volatile unsigned long *)(CAN_ACCEPT_BASE_ADDR + 0x18))
    00936 #define CAN_LUT_ERR     (*(volatile unsigned long *)(CAN_ACCEPT_BASE_ADDR + 0x1C))
    00937
    00938 #define CAN_CENTRAL_BASE_ADDR           0xE0040000
    00939 #define CAN_TX_SR       (*(volatile unsigned long *)(CAN_CENTRAL_BASE_ADDR + 0x00))
    00940 #define CAN_RX_SR       (*(volatile unsigned long *)(CAN_CENTRAL_BASE_ADDR + 0x04))
    00941 #define CAN_MSR         (*(volatile unsigned long *)(CAN_CENTRAL_BASE_ADDR + 0x08))
    00942
    00943 #define CAN1_BASE_ADDR          0xE0044000
    00944 #define CAN1MOD         (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x00))
    00945 #define CAN1CMR         (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x04))
    00946 #define CAN1GSR         (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x08))
    00947 #define CAN1ICR         (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x0C))
    00948 #define CAN1IER         (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x10))
    00949 #define CAN1BTR         (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x14))
    00950 #define CAN1EWL         (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x18))
    00951 #define CAN1SR          (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x1C))
    00952 #define CAN1RFS         (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x20))
    00953 #define CAN1RID         (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x24))
    00954 #define CAN1RDA         (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x28))
    00955 #define CAN1RDB         (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x2C))
    00956
    00957 #define CAN1TFI1        (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x30))
    00958 #define CAN1TID1        (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x34))
    00959 #define CAN1TDA1        (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x38))
    00960 #define CAN1TDB1        (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x3C))
    00961 #define CAN1TFI2        (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x40))
    00962 #define CAN1TID2        (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x44))
    00963 #define CAN1TDA2        (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x48))
    00964 #define CAN1TDB2        (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x4C))
    00965 #define CAN1TFI3        (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x50))
    00966 #define CAN1TID3        (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x54))
    00967 #define CAN1TDA3        (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x58))
    00968 #define CAN1TDB3        (*(volatile unsigned long *)(CAN1_BASE_ADDR + 0x5C))
    00969
    00970 #define CAN2_BASE_ADDR          0xE0048000
    00971 #define CAN2MOD         (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x00))
    00972 #define CAN2CMR         (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x04))
    00973 #define CAN2GSR         (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x08))
    00974 #define CAN2ICR         (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x0C))
    00975 #define CAN2IER         (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x10))
    00976 #define CAN2BTR         (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x14))
    00977 #define CAN2EWL         (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x18))
    00978 #define CAN2SR          (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x1C))
    00979 #define CAN2RFS         (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x20))
    00980 #define CAN2RID         (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x24))
    00981 #define CAN2RDA         (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x28))
    00982 #define CAN2RDB         (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x2C))
    00983
    00984 #define CAN2TFI1        (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x30))
    00985 #define CAN2TID1        (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x34))
    00986 #define CAN2TDA1        (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x38))
    00987 #define CAN2TDB1        (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x3C))
    00988 #define CAN2TFI2        (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x40))
    00989 #define CAN2TID2        (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x44))
    00990 #define CAN2TDA2        (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x48))
    00991 #define CAN2TDB2        (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x4C))
    00992 #define CAN2TFI3        (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x50))
    00993 #define CAN2TID3        (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x54))
    00994 #define CAN2TDA3        (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x58))
    00995 #define CAN2TDB3        (*(volatile unsigned long *)(CAN2_BASE_ADDR + 0x5C))
    00996
    00997
    00998 /* MultiMedia Card Interface(MCI) Controller */
    00999 #define MCI_BASE_ADDR           0xE008C000
    01000 #define MCI_POWER      (*(volatile unsigned long *)(MCI_BASE_ADDR + 0x00))
    01001 #define MCI_CLOCK      (*(volatile unsigned long *)(MCI_BASE_ADDR + 0x04))
    01002 #define MCI_ARGUMENT   (*(volatile unsigned long *)(MCI_BASE_ADDR + 0x08))
    01003 #define MCI_COMMAND    (*(volatile unsigned long *)(MCI_BASE_ADDR + 0x0C))
    01004 #define MCI_RESP_CMD   (*(volatile unsigned long *)(MCI_BASE_ADDR + 0x10))
    01005 #define MCI_RESP0      (*(volatile unsigned long *)(MCI_BASE_ADDR + 0x14))
    01006 #define MCI_RESP1      (*(volatile unsigned long *)(MCI_BASE_ADDR + 0x18))
    01007 #define MCI_RESP2      (*(volatile unsigned long *)(MCI_BASE_ADDR + 0x1C))
    01008 #define MCI_RESP3      (*(volatile unsigned long *)(MCI_BASE_ADDR + 0x20))
    01009 #define MCI_DATA_TMR   (*(volatile unsigned long *)(MCI_BASE_ADDR + 0x24))
    01010 #define MCI_DATA_LEN   (*(volatile unsigned long *)(MCI_BASE_ADDR + 0x28))
    01011 #define MCI_DATA_CTRL  (*(volatile unsigned long *)(MCI_BASE_ADDR + 0x2C))
    01012 #define MCI_DATA_CNT   (*(volatile unsigned long *)(MCI_BASE_ADDR + 0x30))
    01013 #define MCI_STATUS     (*(volatile unsigned long *)(MCI_BASE_ADDR + 0x34))
    01014 #define MCI_CLEAR      (*(volatile unsigned long *)(MCI_BASE_ADDR + 0x38))
    01015 #define MCI_MASK0      (*(volatile unsigned long *)(MCI_BASE_ADDR + 0x3C))
    01016 #define MCI_MASK1      (*(volatile unsigned long *)(MCI_BASE_ADDR + 0x40))
    01017 #define MCI_FIFO_CNT   (*(volatile unsigned long *)(MCI_BASE_ADDR + 0x48))
    01018 #define MCI_FIFO       (*(volatile unsigned long *)(MCI_BASE_ADDR + 0x80))
    01019
    01020
    01021 /* I2S Interface Controller (I2S) */
    01022 #define I2S_BASE_ADDR           0xE0088000
    01023 #define I2S_DAO        (*(volatile unsigned long *)(I2S_BASE_ADDR + 0x00))
    01024 #define I2S_DAI        (*(volatile unsigned long *)(I2S_BASE_ADDR + 0x04))
    01025 #define I2S_TX_FIFO    (*(volatile unsigned long *)(I2S_BASE_ADDR + 0x08))
    01026 #define I2S_RX_FIFO    (*(volatile unsigned long *)(I2S_BASE_ADDR + 0x0C))
    01027 #define I2S_STATE      (*(volatile unsigned long *)(I2S_BASE_ADDR + 0x10))
    01028 #define I2S_DMA1       (*(volatile unsigned long *)(I2S_BASE_ADDR + 0x14))
    01029 #define I2S_DMA2       (*(volatile unsigned long *)(I2S_BASE_ADDR + 0x18))
    01030 #define I2S_IRQ        (*(volatile unsigned long *)(I2S_BASE_ADDR + 0x1C))
    01031 #define I2S_TXRATE     (*(volatile unsigned long *)(I2S_BASE_ADDR + 0x20))
    01032 #define I2S_RXRATE     (*(volatile unsigned long *)(I2S_BASE_ADDR + 0x24))
    01033
    01034
    01035 /* General-purpose DMA Controller */
    01036 #define DMA_BASE_ADDR           0xFFE04000
    01037 #define GPDMA_INT_STAT         (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x000))
    01038 #define GPDMA_INT_TCSTAT       (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x004))
    01039 #define GPDMA_INT_TCCLR        (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x008))
    01040 #define GPDMA_INT_ERR_STAT     (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x00C))
    01041 #define GPDMA_INT_ERR_CLR      (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x010))
    01042 #define GPDMA_RAW_INT_TCSTAT   (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x014))
    01043 #define GPDMA_RAW_INT_ERR_STAT (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x018))
    01044 #define GPDMA_ENABLED_CHNS     (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x01C))
    01045 #define GPDMA_SOFT_BREQ        (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x020))
    01046 #define GPDMA_SOFT_SREQ        (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x024))
    01047 #define GPDMA_SOFT_LBREQ       (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x028))
    01048 #define GPDMA_SOFT_LSREQ       (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x02C))
    01049 #define GPDMA_CONFIG           (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x030))
    01050 #define GPDMA_SYNC             (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x034))
    01051
    01052 /* DMA channel 0 registers */
    01053 #define GPDMA_CH0_SRC      (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x100))
    01054 #define GPDMA_CH0_DEST     (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x104))
    01055 #define GPDMA_CH0_LLI      (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x108))
    01056 #define GPDMA_CH0_CTRL     (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x10C))
    01057 #define GPDMA_CH0_CFG      (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x110))
    01058
    01059 /* DMA channel 1 registers */
    01060 #define GPDMA_CH1_SRC      (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x120))
    01061 #define GPDMA_CH1_DEST     (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x124))
    01062 #define GPDMA_CH1_LLI      (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x128))
    01063 #define GPDMA_CH1_CTRL     (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x12C))
    01064 #define GPDMA_CH1_CFG      (*(volatile unsigned long *)(DMA_BASE_ADDR + 0x130))
    01065
    01066
    01067 /* USB Controller */
    01068 #define USB_INT_BASE_ADDR       0xE01FC1C0
    01069 #define USB_BASE_ADDR           0xFFE0C200              /* USB Base Address */
    01070
    01071 #define USB_INT_STAT    (*(volatile unsigned long *)(USB_INT_BASE_ADDR + 0x00))
    01072
    01073 /* USB Device Interrupt Registers */
    01074 #define DEV_INT_STAT    (*(volatile unsigned long *)(USB_BASE_ADDR + 0x00))
    01075 #define DEV_INT_EN      (*(volatile unsigned long *)(USB_BASE_ADDR + 0x04))
    01076 #define DEV_INT_CLR     (*(volatile unsigned long *)(USB_BASE_ADDR + 0x08))
    01077 #define DEV_INT_SET     (*(volatile unsigned long *)(USB_BASE_ADDR + 0x0C))
    01078 #define DEV_INT_PRIO    (*(volatile unsigned long *)(USB_BASE_ADDR + 0x2C))
    01079
    01080 /* USB Device Endpoint Interrupt Registers */
    01081 #define EP_INT_STAT     (*(volatile unsigned long *)(USB_BASE_ADDR + 0x30))
    01082 #define EP_INT_EN       (*(volatile unsigned long *)(USB_BASE_ADDR + 0x34))
    01083 #define EP_INT_CLR      (*(volatile unsigned long *)(USB_BASE_ADDR + 0x38))
    01084 #define EP_INT_SET      (*(volatile unsigned long *)(USB_BASE_ADDR + 0x3C))
    01085 #define EP_INT_PRIO     (*(volatile unsigned long *)(USB_BASE_ADDR + 0x40))
    01086
    01087 /* USB Device Endpoint Realization Registers */
    01088 #define REALIZE_EP      (*(volatile unsigned long *)(USB_BASE_ADDR + 0x44))
    01089 #define EP_INDEX        (*(volatile unsigned long *)(USB_BASE_ADDR + 0x48))
    01090 #define MAXPACKET_SIZE  (*(volatile unsigned long *)(USB_BASE_ADDR + 0x4C))
    01091
    01092 /* USB Device Command Reagisters */
    01093 #define CMD_CODE        (*(volatile unsigned long *)(USB_BASE_ADDR + 0x10))
    01094 #define CMD_DATA        (*(volatile unsigned long *)(USB_BASE_ADDR + 0x14))
    01095
    01096 /* USB Device Data Transfer Registers */
    01097 #define RX_DATA         (*(volatile unsigned long *)(USB_BASE_ADDR + 0x18))
    01098 #define TX_DATA         (*(volatile unsigned long *)(USB_BASE_ADDR + 0x1C))
    01099 #define RX_PLENGTH      (*(volatile unsigned long *)(USB_BASE_ADDR + 0x20))
    01100 #define TX_PLENGTH      (*(volatile unsigned long *)(USB_BASE_ADDR + 0x24))
    01101 #define USB_CTRL        (*(volatile unsigned long *)(USB_BASE_ADDR + 0x28))
    01102
    01103 /* USB Device DMA Registers */
    01104 #define DMA_REQ_STAT        (*(volatile unsigned long *)(USB_BASE_ADDR + 0x50))
    01105 #define DMA_REQ_CLR         (*(volatile unsigned long *)(USB_BASE_ADDR + 0x54))
    01106 #define DMA_REQ_SET         (*(volatile unsigned long *)(USB_BASE_ADDR + 0x58))
    01107 #define UDCA_HEAD           (*(volatile unsigned long *)(USB_BASE_ADDR + 0x80))
    01108 #define EP_DMA_STAT         (*(volatile unsigned long *)(USB_BASE_ADDR + 0x84))
    01109 #define EP_DMA_EN           (*(volatile unsigned long *)(USB_BASE_ADDR + 0x88))
    01110 #define EP_DMA_DIS          (*(volatile unsigned long *)(USB_BASE_ADDR + 0x8C))
    01111 #define DMA_INT_STAT        (*(volatile unsigned long *)(USB_BASE_ADDR + 0x90))
    01112 #define DMA_INT_EN          (*(volatile unsigned long *)(USB_BASE_ADDR + 0x94))
    01113 #define EOT_INT_STAT        (*(volatile unsigned long *)(USB_BASE_ADDR + 0xA0))
    01114 #define EOT_INT_CLR         (*(volatile unsigned long *)(USB_BASE_ADDR + 0xA4))
    01115 #define EOT_INT_SET         (*(volatile unsigned long *)(USB_BASE_ADDR + 0xA8))
    01116 #define NDD_REQ_INT_STAT    (*(volatile unsigned long *)(USB_BASE_ADDR + 0xAC))
    01117 #define NDD_REQ_INT_CLR     (*(volatile unsigned long *)(USB_BASE_ADDR + 0xB0))
    01118 #define NDD_REQ_INT_SET     (*(volatile unsigned long *)(USB_BASE_ADDR + 0xB4))
    01119 #define SYS_ERR_INT_STAT    (*(volatile unsigned long *)(USB_BASE_ADDR + 0xB8))
    01120 #define SYS_ERR_INT_CLR     (*(volatile unsigned long *)(USB_BASE_ADDR + 0xBC))
    01121 #define SYS_ERR_INT_SET     (*(volatile unsigned long *)(USB_BASE_ADDR + 0xC0))
    01122
    01123 /* USB Host and OTG registers are for LPC24xx only */
    01124 /* USB Host Controller */
    01125 #define USBHC_BASE_ADDR         0xFFE0C000
    01126 #define HC_REVISION         (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x00))
    01127 #define HC_CONTROL          (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x04))
    01128 #define HC_CMD_STAT         (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x08))
    01129 #define HC_INT_STAT         (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x0C))
    01130 #define HC_INT_EN           (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x10))
    01131 #define HC_INT_DIS          (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x14))
    01132 #define HC_HCCA             (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x18))
    01133 #define HC_PERIOD_CUR_ED    (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x1C))
    01134 #define HC_CTRL_HEAD_ED     (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x20))
    01135 #define HC_CTRL_CUR_ED      (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x24))
    01136 #define HC_BULK_HEAD_ED     (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x28))
    01137 #define HC_BULK_CUR_ED      (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x2C))
    01138 #define HC_DONE_HEAD        (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x30))
    01139 #define HC_FM_INTERVAL      (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x34))
    01140 #define HC_FM_REMAINING     (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x38))
    01141 #define HC_FM_NUMBER        (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x3C))
    01142 #define HC_PERIOD_START     (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x40))
    01143 #define HC_LS_THRHLD        (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x44))
    01144 #define HC_RH_DESCA         (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x48))
    01145 #define HC_RH_DESCB         (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x4C))
    01146 #define HC_RH_STAT          (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x50))
    01147 #define HC_RH_PORT_STAT1    (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x54))
    01148 #define HC_RH_PORT_STAT2    (*(volatile unsigned long *)(USBHC_BASE_ADDR + 0x58))
    01149
    01150 /* USB OTG Controller */
    01151 #define USBOTG_BASE_ADDR        0xFFE0C100
    01152 #define OTG_INT_STAT        (*(volatile unsigned long *)(USBOTG_BASE_ADDR + 0x00))
    01153 #define OTG_INT_EN          (*(volatile unsigned long *)(USBOTG_BASE_ADDR + 0x04))
    01154 #define OTG_INT_SET         (*(volatile unsigned long *)(USBOTG_BASE_ADDR + 0x08))
    01155 #define OTG_INT_CLR         (*(volatile unsigned long *)(USBOTG_BASE_ADDR + 0x0C))
    01156 /* On LPC23xx, the name is USBPortSel, on LPC24xx, the name is OTG_STAT_CTRL */
    01157 #define OTG_STAT_CTRL       (*(volatile unsigned long *)(USBOTG_BASE_ADDR + 0x10))
    01158 #define OTG_TIMER           (*(volatile unsigned long *)(USBOTG_BASE_ADDR + 0x14))
    01159
    01160 #define USBOTG_I2C_BASE_ADDR    0xFFE0C300
    01161 #define OTG_I2C_RX          (*(volatile unsigned long *)(USBOTG_I2C_BASE_ADDR + 0x00))
    01162 #define OTG_I2C_TX          (*(volatile unsigned long *)(USBOTG_I2C_BASE_ADDR + 0x00))
    01163 #define OTG_I2C_STS         (*(volatile unsigned long *)(USBOTG_I2C_BASE_ADDR + 0x04))
    01164 #define OTG_I2C_CTL         (*(volatile unsigned long *)(USBOTG_I2C_BASE_ADDR + 0x08))
    01165 #define OTG_I2C_CLKHI       (*(volatile unsigned long *)(USBOTG_I2C_BASE_ADDR + 0x0C))
    01166 #define OTG_I2C_CLKLO       (*(volatile unsigned long *)(USBOTG_I2C_BASE_ADDR + 0x10))
    01167
    01168 /* On LPC23xx, the names are USBClkCtrl and USBClkSt; on LPC24xx, the names are
    01169 OTG_CLK_CTRL and OTG_CLK_STAT respectively. */
    01170 #define USBOTG_CLK_BASE_ADDR    0xFFE0CFF0
    01171 #define OTG_CLK_CTRL        (*(volatile unsigned long *)(USBOTG_CLK_BASE_ADDR + 0x04))
    01172 #define OTG_CLK_STAT        (*(volatile unsigned long *)(USBOTG_CLK_BASE_ADDR + 0x08))
    01173
    01174 /* Note: below three register name convention is for LPC23xx USB device only, match
    01175 with the spec. update in USB Device Section. */
    01176 #define USBPortSel          (*(volatile unsigned long *)(USBOTG_BASE_ADDR + 0x10))
    01177 #define USBClkCtrl          (*(volatile unsigned long *)(USBOTG_CLK_BASE_ADDR + 0x04))
    01178 #define USBClkSt            (*(volatile unsigned long *)(USBOTG_CLK_BASE_ADDR + 0x08))
    01179
    01180 /* Ethernet MAC (32 bit data bus) -- all registers are RW unless indicated in parentheses */
    01181 #define MAC_BASE_ADDR           0xFFE00000 /* AHB Peripheral # 0 */
    01182 #define MAC_MAC1            (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x000)) /* MAC config reg 1 */
    01183 #define MAC_MAC2            (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x004)) /* MAC config reg 2 */
    01184 #define MAC_IPGT            (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x008)) /* b2b InterPacketGap reg */
    01185 #define MAC_IPGR            (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x00C)) /* non b2b InterPacketGap reg */
    01186 #define MAC_CLRT            (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x010)) /* CoLlision window/ReTry reg */
    01187 #define MAC_MAXF            (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x014)) /* MAXimum Frame reg */
    01188 #define MAC_SUPP            (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x018)) /* PHY SUPPort reg */
    01189 #define MAC_TEST            (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x01C)) /* TEST reg */
    01190 #define MAC_MCFG            (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x020)) /* MII Mgmt ConFiG reg */
    01191 #define MAC_MCMD            (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x024)) /* MII Mgmt CoMmanD reg */
    01192 #define MAC_MADR            (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x028)) /* MII Mgmt ADdRess reg */
    01193 #define MAC_MWTD            (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x02C)) /* MII Mgmt WriTe Data reg (WO) */
    01194 #define MAC_MRDD            (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x030)) /* MII Mgmt ReaD Data reg (RO) */
    01195 #define MAC_MIND            (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x034)) /* MII Mgmt INDicators reg (RO) */
    01196
    01197 #define MAC_SA0             (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x040)) /* Station Address 0 reg */
    01198 #define MAC_SA1             (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x044)) /* Station Address 1 reg */
    01199 #define MAC_SA2             (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x048)) /* Station Address 2 reg */
    01200
    01201 #define MAC_COMMAND         (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x100)) /* Command reg */
    01202 #define MAC_STATUS          (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x104)) /* Status reg (RO) */
    01203 #define MAC_RXDESCRIPTOR    (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x108)) /* Rx descriptor base address reg */
    01204 #define MAC_RXSTATUS        (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x10C)) /* Rx status base address reg */
    01205 #define MAC_RXDESCRIPTORNUM (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x110)) /* Rx number of descriptors reg */
    01206 #define MAC_RXPRODUCEINDEX  (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x114)) /* Rx produce index reg (RO) */
    01207 #define MAC_RXCONSUMEINDEX  (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x118)) /* Rx consume index reg */
    01208 #define MAC_TXDESCRIPTOR    (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x11C)) /* Tx descriptor base address reg */
    01209 #define MAC_TXSTATUS        (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x120)) /* Tx status base address reg */
    01210 #define MAC_TXDESCRIPTORNUM (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x124)) /* Tx number of descriptors reg */
    01211 #define MAC_TXPRODUCEINDEX  (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x128)) /* Tx produce index reg */
    01212 #define MAC_TXCONSUMEINDEX  (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x12C)) /* Tx consume index reg (RO) */
    01213
    01214 #define MAC_TSV0            (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x158)) /* Tx status vector 0 reg (RO) */
    01215 #define MAC_TSV1            (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x15C)) /* Tx status vector 1 reg (RO) */
    01216 #define MAC_RSV             (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x160)) /* Rx status vector reg (RO) */
    01217
    01218 #define MAC_FLOWCONTROLCNT  (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x170)) /* Flow control counter reg */
    01219 #define MAC_FLOWCONTROLSTS  (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x174)) /* Flow control status reg */
    01220
    01221 #define MAC_RXFILTERCTRL    (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x200)) /* Rx filter ctrl reg */
    01222 #define MAC_RXFILTERWOLSTS  (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x204)) /* Rx filter WoL status reg (RO) */
    01223 #define MAC_RXFILTERWOLCLR  (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x208)) /* Rx filter WoL clear reg (WO) */
    01224
    01225 #define MAC_HASHFILTERL     (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x210)) /* Hash filter LSBs reg */
    01226 #define MAC_HASHFILTERH     (*(volatile unsigned long *)(MAC_BASE_ADDR + 0x214)) /* Hash filter MSBs reg */
    01227
    01228 #define MAC_INTSTATUS       (*(volatile unsigned long *)(MAC_BASE_ADDR + 0xFE0)) /* Interrupt status reg (RO) */
    01229 #define MAC_INTENABLE       (*(volatile unsigned long *)(MAC_BASE_ADDR + 0xFE4)) /* Interrupt enable reg  */
    01230 #define MAC_INTCLEAR        (*(volatile unsigned long *)(MAC_BASE_ADDR + 0xFE8)) /* Interrupt clear reg (WO) */
    01231 #define MAC_INTSET          (*(volatile unsigned long *)(MAC_BASE_ADDR + 0xFEC)) /* Interrupt set reg (WO) */
    01232
    01233 #define MAC_POWERDOWN       (*(volatile unsigned long *)(MAC_BASE_ADDR + 0xFF4)) /* Power-down reg */
    01234 #define MAC_MODULEID        (*(volatile unsigned long *)(MAC_BASE_ADDR + 0xFFC)) /* Module ID reg (RO) */
    01235
    01236
    01237 /* Some bit-mask definitions - mthomas */
    01238
    01239 /* Timers */
    01240 #define TxIR_MR0_Interrupt (1UL<<0)
    01241 #define TxIR_MR1_Interrupt (1UL<<1)
    01242 #define TxIR_MR2_Interrupt (1UL<<2)
    01243 #define TxIR_MR3_Interrupt (1UL<<3)
    01244 #define TxIR_CR0_Interrupt (1UL<<4)
    01245 #define TxIR_CR1_Interrupt (1UL<<5)
    01246 #define TxIR_CR2_Interrupt (1UL<<6)
    01247 #define TxIR_CR3_Interrupt (1UL<<7)
    01248
    01249 #define TxTCR_Counter_Enable (1UL<<0)
    01250 #define TxTCR_Counter_Reset  (1UL<<1)
    01251
    01252 #define TxMCR_MR0I  (1UL<<0)
    01253 #define TxMCR_MR0R  (1UL<<1)
    01254 #define TxMCR_MR0S  (1UL<<2)
    01255 #define TxMCR_MR1I  (1UL<<3)
    01256 #define TxMCR_MR1R  (1UL<<4)
    01257 #define TxMCR_MR1S  (1UL<<5)
    01258 #define TxMCR_MR2I  (1UL<<6)
    01259 #define TxMCR_MR2R  (1UL<<7)
    01260 #define TxMCR_MR2S  (1UL<<8)
    01261 #define TxMCR_MR3I  (1UL<<9)
    01262 #define TxMCR_MR3R  (1UL<<10)
    01263 #define TxMCR_MR3S  (1UL<<11)
    01264
    01265 /* VIC */
    01266 #define VIC_CHAN_NUM_WDT      0
    01267 #define VIC_CHAN_NUM_UNUSED   1
    01268 #define VIC_CHAN_NUM_ARM_Core_DgbCommRX 2
    01269 #define VIC_CHAN_NUM_ARM_Core_DbgCommTX 3
    01270 #define VIC_CHAN_NUM_Timer0   4
    01271 #define VIC_CHAN_NUM_Timer1   5
    01272 #define VIC_CHAN_NUM_UART0    6
    01273 #define VIC_CHAN_NUM_UART1    7
    01274 #define VIC_CHAN_NUM_PWM1     8
    01275 #define VIC_CHAN_NUM_I2C0     9
    01276 #define VIC_CHAN_NUM_SPI     10
    01277 #define VIC_CHAN_NUM_SSP0    10
    01278 #define VIC_CHAN_NUM_SSP1    11
    01279 #define VIC_CHAN_NUM_PLL     12
    01280 #define VIC_CHAN_NUM_RTC     13
    01281 #define VIC_CHAN_NUM_EINT0   14
    01282 #define VIC_CHAN_NUM_EINT1   15
    01283 #define VIC_CHAN_NUM_EINT2   16
    01284 #define VIC_CHAN_NUM_EINT3   17
    01285 #define VIC_CHAN_NUM_ADC0    18
    01286 #define VIC_CHAN_NUM_I2C1    19
    01287 #define VIC_CHAN_NUM_BOD     20
    01288 #define VIC_CHAN_NUM_Ethernet 21
    01289 #define VIC_CHAN_NUM_USB     22
    01290 #define VIC_CHAN_NUM_CAN     23
    01291 #define VIC_CHAN_NUM_SD_MMC  24
    01292 #define VIC_CHAN_NUM_GP_DMA  25
    01293 #define VIC_CHAN_NUM_Timer2  26
    01294 #define VIC_CHAN_NUM_Timer3  27
    01295 #define VIC_CHAN_NUM_UART2   28
    01296 #define VIC_CHAN_NUM_UART3   29
    01297 #define VIC_CHAN_NUM_I2C2    30
    01298 #define VIC_CHAN_NUM_I2S     31
    01299
    01300 #define VIC_CHAN_TO_MASK(vctm_chan_num__) (1UL<<vctm_chan_num__)
    01301
    01302 #endif  /* __LPC23xx_H */
    01303