/**
  \example eeprom1.cpp 

  This sketch uses #eepromRead and #eepromWrite to read and write one
  byte of EEPROM.  The last value written by a 'wX' packet (whatever
  'X' is) will be read by subsequent 'r' packets, even after the board
  is rebooted or power-cycled.

 */
