# clockConfiguration Struct Reference

The internal hardware parameters associated with a given CPU clock speed. More...

`#include <clock.h>`

## Data Fields
u8 | pllMulM
| PLL multiplier: 6-512, prefer small.
u8 | pllDivN
| PLL predivider: 1-32, prefer small.
u8 | clkDiv
| Clock divider: Even values 2-254.
u8 | mamtim
| MAM clocks: 1+.
u8 | pclkDiv
| Default PCLKDIV: 1,2,4,8.
u8 | pclkMHz
| Default PCLK MHz: Derived value.

## Detailed Description

The internal hardware parameters associated with a given CPU clock speed.

Primarily intended for internal use.

The documentation for this struct was generated from the following file:

- src/include/lpc/clock.h