# PinInfo_s Struct Reference

A description of a single SFB-programmer-visible hardware pin. More...

`#include <SFBPins.h>`

## Data Fields
u8 | portNumber
u8 | bitNumber
| The LPC2000 port number of the pin.
u8 | aliasMode
| The bit number within the port, 0.
u8 | flags
| If >= ALIAS_COUNT, provides alias (alternate index), else default mode.

## Detailed Description

A description of a single SFB-programmer-visible hardware pin.

The attribute is added to force word alignment without union shenanigans...

## Field Documentation

u8 PinInfo_s::aliasMode

The bit number within the port, 0.

.31.

u8 PinInfo_s::bitNumber

The LPC2000 port number of the pin.

0..4.

The documentation for this struct was generated from the following file:

- src/include/SFBPins.h